(footprint "SSD1306"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 12.7 16.51 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "KiCad Tut_SSD1306"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_text user "GND"
		(at -3.81 -5.08 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SDA"
		(at 3.81 -5.08 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC"
		(at -1.27 -5.08 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SCL"
		(at 1.27 -5.08 90)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SSD1306"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" thru_hole rect
		(at -3.81 -10.16)
		(size 2.54 2.54)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -1.27 -10.16)
		(size 2.54 2.54)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 1.27 -10.16)
		(size 2.54 2.54)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.81 -10.16)
		(size 2.54 2.54)
		(drill 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -14 -13.5) (xy 14 -13.5) (xy 14 14.5) (xy -14 14.5)
			)
		)
	)
	(embedded_fonts no)
)
